## Tank pit overview STANDIC Antwerpen

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| TANK PIT | **NR OF TANKS** | **TANK SIZE(S) IN M3** | **MS/DX-SS** | **HEIGHT IN M** | **EXPECTED TO BE OPERATIONAL** |
|  | | | | | |
| 1+2 | 19 | 750 | DX-SS | 14 | OPERATIONAL |
| 3 | 12 | 500 | DX-SS | 14 | OPERATIONAL |
| 4+5+6+7 | 40 | 1250 | DX-SS | 24 | OPERATIONAL |
| 8 | 8 | 2000 | 2500 | 3500 | MS | 24 | OPERATIONAL |
|  | | | | | |
| 9 | 10 | 1500 | DX-SS | 24 | OPERATIONAL |
| 10 | 8 | 2000 | 2500 | 3000 | DX-SS | 24 | OPERATIONAL |
| 11 | 10 | 1500 | 1750 | DX-SS | 24 | OPERATIONAL |
| 12 | 10 | 1500 | DX-SS | 24 | OPERATIONAL |
| 13 | 8 | 2000 | 3000 | DX-SS | 24 | OPERATIONAL |
|  | | | | | |
| 14 | 20 | 500 | DX-SS | 15 | WILL FOLLOW |
| 15 | 22 | 750 | 1000 | DX-SS | 20 | WILL FOLLOW |
| 16 | 10 | 1750 | DX-SS | 24 | WILL FOLLOW |
| 17 | 8 | 2000 | 2500 | 3000 | DX-SS | 24 | WILL FOLLOW |

All tanks will be insulated and suitable for heating, blanketing and mixing.

Please contact our sales department ([Sales@standic.com](mailto:Sales@standic.com)) for further information.